Stanford Exploration Project, Report DATALIB, January 16, 2002, pages 1–37

Amoco 3D-Land

Robert G. Clapp^1

ABSTRACT Amoco 3D-Land dataset

AMOCO GOM DATA

Raw Data tape Velocity Model Unknown Stack /data_3d/amoco-3dland/stack.H Usage Lumley Geometry

                ********** amoco_sort.H ************
          4 -esize Synched data_format-xdr_float
-----------------------------------------------------------------
n1=1000 o1=0.000000 d1=0.002000 label1=time
n2=606097 o2=1.000000 d2=1.000000 label2=trace_number
Data: in=/data_3d/amoco-3dland/amoco_sort.H@
     606097 elements, 2424388000 bytes in data file
-----------------------------------------------------------------
keynumber=1 keytype=scalar_int keyname=sx
keynumber=2 keytype=scalar_int keyname=sy
keynumber=3 keytype=scalar_int keyname=gx
keynumber=4 keytype=scalar_int keyname=gy
keynumber=5 keytype=scalar_int keyname=cdp
keynumber=6 keytype=scalar_int keyname=offset
keynumber=7 keytype=scalar_int keyname=sstat
keynumber=8 keytype=scalar_int keyname=gstat
keynumber=9 keytype=scalar_float keyname=s_x
keynumber=10 keytype=scalar_float keyname=g_x
keynumber=11 keytype=scalar_float keyname=s_y
keynumber=12 keytype=scalar_float keyname=g_y
keynumber=13 keytype=scalar_float keyname=cmp_x
keynumber=14 keytype=scalar_float keyname=cmp_y

1email: bob@sep.stanford.edu 1

2 Clapp SEP–DATALIB

keynumber=15 keytype=scalar_float keyname=offset_x
keynumber=16 keytype=scalar_float keyname=offset_y
keynumber=17 keytype=scalar_float keyname=aoffset
keynumber=18 keytype=scalar_float keyname=azimuth
keynumber=19 keytype=scalar_int keyname=data_record_number
n2=606097 o2=1.000000 d2=1.000000 label2=trace_number
Headers in=/data_3d/amoco-3dland/amoco_sort.H@@@
   11515843 elements, 46063372 bytes in data file
-----------------------------------------------------------------
grid axis2 n2=7 o2=1.000000 d2=1.000000 label2=trace_in_bin
grid axis3 n3=45 o3=-330.000000 d3=100.000000 label3=cmp_x
grid axis4 n4=63 o4=500.000000 d4=100.000000 label4=cmp_y
grid axis5 n5=9 o5=-400.000000 d5=100.000000 label5=offset_xgrid axis6 n6=117 o6=-
5800.000000 d6=100.000000 label6=offset_y
Grid in=/data_3d/amoco-3dland/amoco_sort.H@@@@@
   20896785 elements, 83587140 bytes in data file
-----------------------------------------------------------------
-----------------------------------------------------------------

Problem History of Data ???????? Preprocessing ???????? Proprietary Considerations ????????

REFERENCES

Figure 1: CMP gather amoco-3dland-cmp [ER]

Figure 2: Shot geometry amoco-3dland-shot [ER]

Figure 3: Near offset amoco-3dland-near [ER]

Figure 4: Fold-offset amoco-3dland-fold-off [ER]

Figure 5: Fold-cmp amoco-3dland-fold-cmp [ER]

172 SEP–DATALIB